			rtg.library:
This avoid mousetrails and redraw problems in picasso96 on JIT
copy it in libs:pacasso96

			picasso96fix
This allow larger Screen Width than 1024 
start it BEFORE the loadwb instruction in startup-sequence

			uae_german
This is a German keymap to reach @\~{[]} with ALT-GR like windows
Copy it in devs/keymaps and choose it in the keymap-prefs


                         uae/uae.audio 
This is the AHI Drivers.This allow support for 44.1khz 16Bit and 32khz
Make sure you set in uaeprefs 16bit and stereo output  when using this
The outputrate is automatic set correct
Selelct in AHIPREFS or application the uae audiomode to use it 
Recommend you use outrate 32khz or 44.1 khz in Applikation to avoid
rate converting(no hifi Quality converting for now done) 
If a apllication use paula (AHI) another application cannot use 
uae AHI at same time. 
 
copy uae       to devs:audiomodes
copy uae.audio to devs:ahi


NOTICE:THE AHI DRIVER WORK NOT WITH LINUX UAE (Soundquality is then 
a little worser than paula)and not usefull there
